User's Guide
Reference Manual
Release Notes
PDF
Top

Diameter
Release Notes
Version 1.11.1

Expand All
Contract All

Chapters

- Release Notes
  - Top of chapter
  - diameter 1.11.1
  - diameter 1.11
  - diameter 1.10
  - diameter 1.9.2
  - diameter 1.9.1
  - diameter 1.9
  - diameter 1.8
  - diameter 1.7.1
  - diameter 1.7
  - diameter 1.6
  - diameter 1.5
  - diameter 1.4.4
  - diameter 1.4.3
  - diameter 1.4.2
  - diameter 1.4.1.1
  - diameter 1.4.1
  - diameter 1.4
  - diameter 1.3.1
  - diameter 1.3
  - diameter 1.2
  - diameter 1.1
  - diameter 1.0
  - diameter 0.10
  - diameter 0.9

# 1 Release Notes

Releases are listed in reverse chronological order, most recent first.

### 1.1 diameter 1.11.1

#### Fixed Bugs and Malfunctions

- Fix request table leaks

  The End-to-End and Hop-by-Hop identifiers of outgoing Diameter requests are stored in a table in order for the caller to be located when the corresponding answer message is received. Entries were orphaned if the handler was terminated by an exit signal as a consequence of actions taken by callback functions, or if callbacks modified identifiers in retransmission cases.

  Own Id: OTP-13137

### 1.2 diameter 1.11

#### Fixed Bugs and Malfunctions

- Fix relay encode of nested, Grouped AVPs.

  A fault in OTP-12475 caused encode to fail if the first AVP in a Grouped AVP was itself Grouped.

  Own Id: OTP-12879 Aux Id: OTP-12475

- Match acceptable peer addresses case insensitively.

  Regular expressions passed in an 'accept' tuple to diameter_tcp or diameter_sctp inappropriately matched case.

  Own Id: OTP-12902

- Fix diameter_watchdog function clause.

  OTP-12912 introduced an error with accepting transports setting {restrict_connections, false}, causing processes to fail when peer connections were terminated.

  Own Id: OTP-12969

#### Improvements and New Features

- Don't report 5005 (DIAMETER_AVP_MISSING) errors unnecessarily.

  An AVP whose decode failed was reported as missing, despite having been reported with another error as a consequence of the failure.

  Own Id: OTP-12871

- Improve decode performance.

  The time required to decode a message increased quadratically with the number of AVPs in the worst case, leading to extremely long execution times.

  Own Id: OTP-12891

- Improve watchdog and statistics performance.

  Inefficient use of timers contributed to poor performance at high load, as did ordering of the table statistics are written to.

  Own Id: OTP-12912

- Add service_opt() strict_mbit.

  There are differing opinions on whether or not reception of an arbitrary AVP setting the M-bit is an error. The default interpretation is strict: if a command grammar doesn't explicitly allow an AVP setting the M-bit then reception of such an AVP is regarded as an error. Setting {strict_mbit, false} disables this check.

  Own Id: OTP-12947

### 1.3 diameter 1.10

#### Fixed Bugs and Malfunctions

- Fix decode of Grouped AVPs containing errors.

  RFC 6733 says this of Failed-AVP in 7.5:

    In the case where the offending AVP is embedded within a Grouped AVP, the Failed-AVP MAY contain the grouped AVP, which in turn contains the single offending AVP. The same method MAY be employed if the grouped AVP itself is embedded in yet another grouped AVP and so on. In this case, the Failed-AVP MAY contain the grouped AVP hierarchy up to the single offending AVP. This enables the recipient to detect the location of the offending AVP when embedded in a group.

  It says this of DIAMETER_INVALID_AVP_LENGTH in 7.1.5:

    The request contained an AVP with an invalid length. A Diameter message indicating this error MUST include the offending AVPs within a Failed-AVP AVP. In cases where the erroneous AVP length value exceeds the message length or is less than the minimum AVP header length, it is sufficient to include the offending AVP header and a zero filled payload of the minimum required length for the payloads data type. If the AVP is a Grouped AVP, the Grouped AVP header with an empty payload would be sufficient to indicate the offending AVP. In the case where the offending AVP header cannot be fully decoded when the AVP length is less than the minimum AVP header length, it is sufficient to include an offending AVP header that is formulated by padding the incomplete AVP header with zero up to the minimum AVP header length.

  The AVPs placed in the errors field of a diameter_packet record are intended to be appropriate for inclusion in a Failed-AVP, but neither of the above paragraphs has been followed in the Grouped case: the entire faulty AVP (non-faulty components and all) has been included. This made it difficult to identify the actual faulty AVP in all but simple cases.

  The decode is now adapted to the RFC, and implements the suggested single faulty AVP, nested in as many Grouped containers as required.

  Own Id: OTP-12721

- Fix SCTP problems on Solaris.

  The allocation of association ids in Solaris was in conflict with an assumption made in diameter_sctp, resulting in failures when accepting multiple peer connections.

  Own Id: OTP-12768

- Fix start order of alternate transports.

  A transport configured with diameter:add_transport/2 can be passed multiple transport_module/transport_config tuples in order to specify alternate configuration, modules being attempted in order until one succeeds. This is primarily for the connecting case; for example, to allow a transport to be configured to first attempt connection over SCTP, and then TCP in case SCTP fails. Multiple module tuples can be paired with a single config tuple, but in this case the start order was reversed relative to the order in which the modules were specifed.

  Own Id: OTP-12851

#### Improvements and New Features

- Change license text from Erlang Public License to Apache Public License v2.

  Own Id: OTP-12845

### 1.4 diameter 1.9.2

#### Fixed Bugs and Malfunctions

- Fix broken relay counters.

  OTP-12654 in OTP 17.5.3 broke counters in the case of answer messages received in the relay application. Counters were accumulated as unknown messages or no_result_code instead of as relayed messages on the intended Result-Code and 'Experimental-Result' tuples.

  Own Id: OTP-12741

- Fix diameter_sctp listener race.

  An oversight in OTP-12428 made it possible to start a transport process that could not establish associations.

  Own Id: OTP-12744

### 1.5 diameter 1.9.1

#### Known Bugs and Problems

- Don't leave extra bit in decoded AVP data.

  OTP-12074 in OTP 17.3 missed one case: a length error on a trailing AVP unknown to the dictionary in question.

  Own Id: OTP-12642

- Don't confuse Result-Code and Experimental-Result.

  The errors field of a decoded diameter_packet record was populated with a Result-Code AVP when an Experimental-Result containing a 3xxx Result-Code was received in an answer not setting the E-bit. The correct AVP is now extracted from the incoming message.

  Own Id: OTP-12654

- Don't count on unknown Application Id.

  OTP-11721 in OTP 17.1 missed the case of an Application Id not agreeing with that of the dictionary in question, causing counters to be accumulated on keys containing the unknown id.

  Own Id: OTP-12701

### 1.6 diameter 1.9

#### Fixed Bugs and Malfunctions

- Don't discard outgoing answers unnecessarily.

  Answers missing a Result-Code AVP or setting an E-bit inappropriately were discarded even if encode was successful.

  Own Id: OTP-11492

- Increase supervision timeouts.

  At diameter application shutdown, DPR could be omitted on open peer connections because of short supervision timeouts.

  Own Id: OTP-12412

- Fix retransmission of messages sent as header/avps list.

  Extracting End-to-End and Hop-by-Hop Identifiers resulted in a function clause error, resulting in a handle_error callback.

  Own Id: OTP-12415

- Fix diameter_avp decode of Grouped AVPs having decode errors.

  Components of such an AVP were not extracted, causing it to be represented by a single diameter_avp record instead of the intended list.

  Dictionary files must be recompiled for the fix to have effect.

  Own Id: OTP-12475

- Fix ordering of AVPs in relayed messages.

  The order was reversed relative to the received order, with a Route-Record AVP prepended.

  Thanks to Andrzej Trawiński.

  Own Id: OTP-12551

- Fix issues with DiameterURI encode/decode.

  RFC 6773 changed the default port and transport, but the RFC 3588 defaults were used even if the RFC 6733 common dictionary was in use. The RFC 3588 defaults are now only used when the common dictionary is diameter_gen_base_rfc3588.

  Both RFC 3588 and 6733 disallow transport=udp;protocol=diameter. Encode of the combination now fails.

  Decode of ports numbers outside the range 0-65535 and fully qualified domain names longer than 255 octets now fails.

  Note that RFC 3588 is obsolete, and that there is a diameter_gen_base_rfc6733. The change in defaults is a potential interoperability problem when moving to RFC 6733 with peers that do not send all URI components. The fact that 6733 allows 5xxx result codes in answer messages setting the E-bit, which RFC 3588 doesn't, is another.

  Own Id: OTP-12589

#### Improvements and New Features

- Add service_opt() string_decode.

  To disable the decode of potentially large binaries to string. This prevents large strings from being copied when incoming Diameter messages are passed between processes, a vulnerability that can lead to memory being exhausted given sufficiently malicious peers.

  The value is a boolean(), true being the default for backwards compatibility. Setting false causes both diameter_caps records and decoded messages to contain binary() in relevant places that previously had string(): diameter_app(3) callbacks need to be prepared for the change.

  The Diameter types affected are OctetString and the derived types UTF8String, DiameterIdentity, DiameterURI, IPFilterRule, and QoSFilterRule. Time and Address are unaffected.

  Own Id: OTP-11952

- Add transport_opt() pool_size.

  To allow for pools of accepting transport processes, which can better service multiple simultaneous peer connections. The option can also be used with connecting transports, to establish multiple connections to the same peer without having to configure multiple transports.

  Own Id: OTP-12428

- Allow DPR to be sent with diameter:call/4.

  It has been possible to send, but the answer was regarded as unsolicited and discarded. DPA now causes the transport process in question to be terminated, as for DPR that diameter itself sends.

  Own Id: OTP-12542

- Discard requests after DPR.

  RFC 6733 is imprecise, but the tone is that messages received after DPR are an exception to be dealt with only because of the possibility of unordered delivery over SCTP. As a consequence, and because a request following DPR is unlikely to be answered due to the impending loss of the peer connection, discard outgoing requests following an outgoing or incoming DPR. Incoming requests are also discarded, with the exception of DPR itself. Answers are sent and received as usual.

  Own Id: OTP-12543

- Add transport_opt() dpr_timeout.

  To cause a peer connection to be closed following an outgoing DPA when the peer fails to do so. It is the recipient of DPA that should close the connection according to RFC 6733.

  Own Id: OTP-12609

- Add service_opt() incoming_maxlen.

  To bound the expected size of incoming Diameter messages. Messages larger than the specified number of bytes are discarded, to prevent a malicious peer from generating excessive load.

  Own Id: OTP-12628

### 1.7 diameter 1.8

#### Fixed Bugs and Malfunctions

- Fix remote diameter_request table leak.

  An outgoing request whose pick_peer callback selected a transport on another node resulted in an orphaned table entry on that node.

  Own Id: OTP-12196

- Fix handling of 3xxx Result-Code without E-bit.

  OTP-12233 broke the population of the errors field of the diameter_packet record when an incoming request with an E-bit/Result-Code mismatch was detected, causing a 4-tuple to be inserted as Result-Code in a diameter_avp record.

  Own Id: OTP-12233

- Fix ignored connect timer.

  There are two timers governing the establishment of peer connections: connect_timer and watchdog_timer. The former is the RFC 6733 Tc timer, and is used at initial connection establishment. The latter is RFC 3539 TwInit, and is used for connection reestablishment. A connecting transport erroneously used watchdog_timer in both cases.

  Own Id: OTP-12281 Aux Id: seq12728

#### Improvements and New Features

- Order candidate peers in pick_peer callbacks.

  The order of candidate peers presented to a diameter_app(3) pick_peer callback has previously not been documented, but there are use cases that are simplified by an ordering. The order is now determined by the filter.

  Own Id: OTP-12308

### 1.8 diameter 1.7.1

#### Fixed Bugs and Malfunctions

- Don't leave extra bit in decoded AVP data.

  An extra bit could be communicated in the data field of a diameter_avp record in the case of length errors. Of no consequence for code using the record encoding of Diameter messages, but code examining diameter_avp records would see this bit.

  Dictionary files must be recompiled for the fix to have effect.

  Own Id: OTP-12074

- Fix counting of outgoing requests and answers setting the E-bit.

  OTP-11721 broke these counters for all outgoing requests except DWR, and caused answers setting the E-bit to be counted as unknown messages.

  Own Id: OTP-12080

- Fix Failed-AVP decode.

  The best-effort decode only worked for AVPs in the common dictionary, not for those in the dictionary of the application identified in the Diameter Header of the answer message in question.

  Failed-AVP in an answer decoded with the RFC 3588 common dictionary (diameter_gen_base_rfc3588) was regarded as an error. The RFC 6733 dictionary was unaffected.

  Dictionary files must be recompiled for the fix to have effect.

  Own Id: OTP-12094

### 1.9 diameter 1.7

#### Fixed Bugs and Malfunctions

- Improve robustness.

  Counters returned by diameter:service_info/2 now only count messages known to the dictionary in question, so that an attacker cannot cause arbitrarily many counters to be created.

  Messages to the Erlang log have been minimized, and those related to traffic have been removed entirely since an attacker could cause a node to be logged to death. Consequently, the default answer_errors configuration has been changed from report to discard. A service needs to be restarted for the change in default to take effect.

  Own Id: OTP-11721

- Fix request table leak.

  Outgoing Diameter requests are stored in a table until an answer is received or times out. Calling diameter:stop_service/1 before this took place would orphan the entries, resulting in a memory leak.

  Own Id: OTP-11893

- Fix broken SCTP transport.

  OTP-11593 caused the sending of answer messages over SCTP to fail.

  Own Id: OTP-11901 Aux Id: OTP-11593

- Fix watchdog process leak.

  A failed capabilities exchange on a listening transport would orphan a process, causing a memory leak.

  Own Id: OTP-11934

- Fix incorrect handling of incoming DPR.

  In the case of a listening transport, a reconnection by a peer following DPR could transition the watchdog state to REOPEN instead of OKAY.

  Own Id: OTP-11938

- Fix handling of AVP length errors on unknown AVPs.

  An AVP (Header) length that pointed past the end of the message was not flagged as a 5014 error in this case. Moreover, encoding such an AVP in the Failed-AVP of an answer message as a consequence of other errors (eg. M-bit, resulting in 5001) failed if the AVP contained a complete header.

  Dictionary files must be recompiled for the fix to have effect.

  Own Id: OTP-11946

- Fix broken check in dictionary compilation.

  That an AVP specified in the content of a @codecs or @custom_types section was undefined went undetected, causing compilation to fail when attempting to lookup the AVP's type.

  Own Id: OTP-11958

#### Improvements and New Features

- Add result code counters for CEA, DWA, and DPA.

  In addition to the existing result code counters on other answer messages.

  Own Id: OTP-11891

- Add best-effort decode of AVPs within Failed-AVP.

  OTP-11007 disabled the decode of AVPs in Failed-AVP since errors could cause the decode of Failed-AVP itself to fail. Component AVPs are now decoded if possible, otherwise not. AVPs of type Grouped are decoded as much as possible, as deeply as possible.

  Dictionary files must be recompiled for the fix to have effect.

  Own Id: OTP-11936 Aux Id: OTP-11007

- Add counters for encode errors in outgoing Diameter messages.

  In addition to the existing counters on decode errors. The latter now count independently of result codes in answer messages since decode errors do not preclude the presence of a result code.

  Own Id: OTP-11937

### 1.10 diameter 1.6

#### Fixed Bugs and Malfunctions

- Add missing check at dictionary compilation.

  In particular, that an AVP defined as having type Grouped in an @avp_types section has a corresponding definition in a @grouped section.

  Own Id: OTP-11561

- Correct documentation on the setting of Origin-State-Id

  It was incorrectly stated that the AVP would be set in an outgoing DPR/DPA.

  Own Id: OTP-11583

- Change interface for communicating outbound stream id to diameter_sctp

  The module uses the transport_data field of record diameter_packet to communicate the stream on which the an incoming message is received and on which an outgoing message should be sent, the previous interface being that both are communicated as a tuple of the form {stream, Id}. However, since diameter retains the value of an incoming request's transport_data unless the corresponding answer message specifies otherwise, the behaviour in this case is to send an answer on the outbound stream with the same identifier as the that of the inbound stream on which the request was received. If the inbound stream id is greater than or equal to the number of outbound streams then this is guaranteed to fail, causing the transport process in question to terminate. There is no relationship between inbound and outbound stream identifiers so diameter_sctp's imposition of one is simply wrong.

  Outbound stream ids are now communicated with a different tuple: {outstream, Id}, interpreted modulo the number of outbound streams. Thus, retention of an inbound request's transport_data has no effect on the selection of an outbound stream.

  The change in interface is not strictly backwards compatible because of the new atom for the outbound stream. However, as there is currently no documented way of obtaining the available number of outbound streams for a peer connection, there is no way for a client to have known the range of ids from which it could reliably have chosen with the previous interface, so any setting of the outbound stream has probably been unintentional. Not explicitly specifying an outbound stream now results in a round-robin selection.

  Thanks to Sharmila Pillai for reporting the problem.

  *** POTENTIAL INCOMPATIBILITY ***

  Own Id: OTP-11593

- Fix unicode path failure in diameter_make:codec/2.

  A dictionary path containing a unicode codepoint > 255 caused the function to fail.

  Own Id: OTP-11655

- Fix 'accept' config to diameter_sctp.

  OTP-10893 added support for {accept, Match} tuples to specify addresses or regexps that should be matched against peer addresses to decide whether or not a newly established association should be retained, but this hasn't been functional in the SCTP case because of missing support in inet(3).

  The display of both local and peer addresses in diameter:service_info/2 output has also been corrected.

  Own Id: OTP-11661 Aux Id: OTP-10229

- Be lenient with the M-bit in Grouped AVPs.

  RFC 6733 says this, in 4.4:

    Receivers of a Grouped AVP that does not have the 'M' (mandatory) bit set and one or more of the encapsulated AVPs within the group has the 'M' (mandatory) bit set MAY simply be ignored if the Grouped AVP itself is unrecognized. The rule applies even if the encapsulated AVP with its 'M' (mandatory) bit set is further encapsulated within other sub-groups, i.e., other Grouped AVPs embedded within the Grouped AVP.

  The first sentence is mangled but take it to mean this:

    An unrecognized AVP of type Grouped that does not set the 'M' bit MAY be ignored even if one of its encapsulated AVPs sets the 'M' bit.

  This is a bit of a non-statement since if the AVP is unrecognized then its type is unknown. We therefore don't know that its data bytes contain encapsulated AVPs, so can't but ignore any of those that set the M-bit. Doing anything else when the type *is* known would be inconsistent.

  OTP-11087 (R16B03) caused the M-bit on any unrecognized AVP to be regarded as an error, unrecognized being taken to mean "not explicitly defined as a member of its container". (That is, an AVP that can't be packed into a dedicated record field, which is slightly stronger than "not defined".) This fixed the original intention for top-level AVPs but broke the required leniency for Grouped AVPs whose type is known. This leniency is now restored.

  Note that dictionary files need to be recompiled for the change to have effect.

  Thanks to Rory McKeown for reporting the problem.

  Own Id: OTP-11675 Aux Id: OTP-11087

- Fix pick_peer case clause failure.

  In the case of {call_mutates_state, true} configuration on the service in question, any peer selection that failed to select a peer resulted in a case clause failure. This was noticed in the case of a peer failover in which an alternate peer wasn't available.

  Own Id: OTP-11789

### 1.11 diameter 1.5

#### Improvements and New Features

- Rename reconnect_timer to connect_timer.

  The former is still accepted for backwards compatibility, but the name is misleading given the semantics of the timer.

  Own Id: OTP-11168

- Extend diameter_make(3).

  Dictionaries can now be compiled from strings, not just filesystem paths, and results can be returned instead of written to the filesystem.

  Own Id: OTP-11348

- Remove hardcoding of diameter_base as @prefix on dictionaries for application id 0.

  Own Id: OTP-11361

### 1.12 diameter 1.4.4

#### Fixed Bugs and Malfunctions

- Fix setting of End-to-End and Hop-by-Hop Identifiers in outgoing DWA.

  Broken by OTP-11184, which caused the identifiers to be set anew, discarding the values from the incoming DWR.

  Own Id: OTP-11367

- Fix handling of 5014, DIAMETER_INVALID_AVP_LENGTH.

  The error was detected as 5004, DIAMETER_INVALID_AVP_VALUE, for some Diameter types, in which case an AVP length that pointed past the end of a message resulted in encode failure.

  Own Id: OTP-11395

### 1.13 diameter 1.4.3

#### Fixed Bugs and Malfunctions

- Fix UTF8String encode.

  Encode now accepts any nested list of codepoints and binaries. A list containing a binary was previously misinterpreted and the documentation was incomplete.

  Own Id: OTP-11172

- Ensure DWR isn't sent immediately after DWA.

  This was possible if the timing was unfortunate. An incoming DWR now properly resets the watchdog timer.

  Own Id: OTP-11184

- Fix faulty encode of Failed-AVP

  Reception of a CER, DWR or DPR that has decode failures caused encode of the corresponding answer message to fail.

  Own Id: OTP-11293

- Fix broken service_opt() spawn_opt.

  The option was ignored.

  Own Id: OTP-11299

### 1.14 diameter 1.4.2

#### Fixed Bugs and Malfunctions

- Fix handling of 5014 (INVALID_AVP_LENGTH) errors.

  This was in some cases reported as 3009 (INVALID_AVP_BITS).

  Note that the correction is partially implemented in modules generated by diameterc(1): a dictionary file must be recompiled for the correction to apply to any messages it defines.

  Own Id: OTP-11007

- Fix faulty capitalization in release notes.

  Diameter = the protocol.
  diameter = the Erlang application.

  Own Id: OTP-11014

- Fix watchdog memory leak.

  Entries were not removed from a service-specific ets table, causing them to be orphaned at connection reestablishment for listening transports, and diameter:remove_transport/2 for both listening and connecting transports.

  The fault was introduced by OTP-10692 in diameter-1.4.1 (R16B).

  Own Id: OTP-11019 Aux Id: OTP-10692

- Fix decode failure on AVP Length < 8.

  The failure caused the message in question to be discarded.

  Own Id: OTP-11026

- Respect Host-IP-Address configuration.

  Addresses returned from a transport module were always used to populate Host-IP-Address AVP's in an outgoing CER/CEA, which precluded the sending of a VIP address. Transport addresses are now only used if Host-IP-Address is unspecified.

  Own Id: OTP-11045

- Fix mkdir race.

  Install could fail if examples/code and examples/dict were created in parallel. Noticed on FreeBSD.

  Own Id: OTP-11051

- Fix recognition of 5001 on mandatory AVP's.

  An AVP setting the M-bit was not regarded as erroneous if it was defined in the dictionary in question and its container (message or Grouped AVP) had an 'AVP' field. It's now regarded as a 5001 error (AVP_UNSUPPORTED), as in the case that the AVP is not defined.

  Note that the correction is partially implemented in modules generated by diameterc(1): a dictionary file must be recompiled for the correction to apply to any messages it defines.

  Own Id: OTP-11087

- Fix setting of Failed-AVP on handle_request {answer_message, 5xxx} return.

  Failed-AVP was never in the outgoing answer-message. It is now set with the AVP from the first entry with the specified Result-Code in the errors field of the incoming diameter_packet, if found.

  Own Id: OTP-11092

- Fix watchdog function_clause

  A listening transport on a service that allowed multiple connections to the same peer could result in a function_clause error in module diameter_watchdog. The resulting crash was harmless but unseemly.

  Thanks to Aleksander Nycz.

  Own Id: OTP-11115

- Fix population of Failed-AVP.

  In cases in which diameter populated this AVP, many values were sent instead of one as suggested by RFC 6733. This was partially corrected by OTP-11007.

  Own Id: OTP-11127 Aux Id: OTP-11007

- Fix list-valued Vendor-Specific-Application-Id config

  R16B (specifically, OTP-10760) broke the handling of such configuration, resulting in a function clause error if the list was not of length 3, and faulty interpretation of the list's contents otherwise. Only record-valued configuration was properly interpreted.

  Own Id: OTP-11165

#### Improvements and New Features

- Allow peer connections to be shared between Erlang nodes for the purpose of sending outgoing requests.

  A diameter_app(3) pick_peer/4 callback gets a list of remote candidates as argument, allowing a callback on one node to select a transport connection established on another node. The service_opt() share_peers controls the extent to which local connections are shared with remote nodes. The service_opt() use_shared_peers controls the extent to which connections shared from remote nodes are utilized on the local node.

  Own Id: OTP-9610

- Allow listening diameter_{tcp,sctp} transports to be configured with remote addresses.

  Option 'accept' allows remote addresses to be configured as tuples or regular expressions. Remote addresses are matched against the configured values at connection establishment, any non-matching address causing the connection to be aborted.

  Own Id: OTP-10893

- Detect more transport_opt() configuration errors at diameter:add_transport/2.

  Many errors would previously not be detected until transport start, diameter:add_transport/2 returning 'ok' but transport connections failing to be established. An error tuple is now returned.

  Own Id: OTP-10972

- Make explicit local address configuration optional in diameter_tcp:start/3.

  The default address (as determined by gen_tcp) is now used when a local address is not explicitly configured.

  Own Id: OTP-10986

- Improve handling of unrecognized service options.

  Such options were silently ignored by diameter:start_service/2. An error tuple is now returned.

  Own Id: OTP-11017

- Don't send default Inband-Security-Id in CER/CEA.

  RFC 6733 recommends against the use of Inband-Security-Id. Only send a value that differs from the default, NO_INBAND_SECURITY = 0.

  Own Id: OTP-11050

- Make spawn options for request processes configurable.

  Own Id: OTP-11060

### 1.15 diameter 1.4.1.1

#### Fixed Bugs and Malfunctions

- Fix broken Vendor-Specific-Application-Id configuration.

  RFC 6733 changed the definition of this Grouped AVP, changing the arity of Vendor-Id from 1* to 1. A component Vendor-Id can now be either list- or integer-valued in service and transport configuration, allowing it to be used with both RFC 3588 and RFC 6733 dictionaries.

  Own Id: OTP-10942

#### Improvements and New Features

- Add transport_opt() watchdog_config to allow non-standard behaviour of the watchdog state machine.

  This can be useful during test but should not be used on nodes that must conform to RFC 3539.

  Own Id: OTP-10898

### 1.16 diameter 1.4.1

#### Fixed Bugs and Malfunctions

- Fix erroneous watchdog transition from DOWN to INITIAL.

  This transition took place when a peer connection was reestablished following a failed capabilities exchange. RFC 3539 requires DOWN to transition into REOPEN.

  Own Id: OTP-10692

#### Improvements and New Features

- Add application_opt() request_errors to make the handling of incoming requests containing decode errors configurable.

  The value 'callback' ensures that a handle_request callback takes place for all such requests, the default being for diameter to answer 3xxx series errors itself.

  Own Id: OTP-10686

- Add transport_opt() length_errors.

  The value determines how messages received over the transport interface with an incorrect Message Length are dealt with.

  Own Id: OTP-10687

- Add commentary on RFC 6733 to Standards Compliance chapter of the User's Guide.

  Own Id: OTP-10688

- Allow a 5xxx result code in an answer-message on peer connections using the RFC 6733 common dictionary.

  RFC 6733 allows this while RFC 3588 does not. A handle_request callback can return {answer_message, 3000..3999|5000..5999} in the simplest case.

  Own Id: OTP-10759

- Add dictionaries for RFC 6733.

  Both the common and accounting dictionaries differ from their RFC 3588 counterparts, which is reflected in generated record definitions. Application configuration on a service or transport determines the dictionary that will be used on a given peer connection.

  Own Id: OTP-10760

- Allow a handle_request callback to control diameter's setting of Result-Code and Failed-AVP.

  Setting errors = false in a returned #diameter_packet{} disables the setting.

  Own Id: OTP-10761

### 1.17 diameter 1.4

#### Fixed Bugs and Malfunctions

- Add registered server names to the app file.

  Own Id: OTP-10442

- Fix #diameter_header{} handling broken by OTP-10445.

  The fault caused the the header of a [Header | Avps] request to be ignored if both end_to_end_id and hop_by_hop_id were undefined.

  Own Id: OTP-10609

- Fix error handling for handle_request callback.

  A callback that returned a #diameter_packet{} would fail if the incoming request had decode errors.

  Own Id: OTP-10614

- Fix timing of service start event.

  The event did not necessarily precede other events as documented.

  Own Id: OTP-10618

- Fix setting of header T flag at peer failover.

  The flag is now set in the diameter_header record passed to a prepare_retransmit callback.

  Own Id: OTP-10619

- Fix sending of CER/CEA timeout event at capx_timeout.

  The event was not sent as documented.

  Own Id: OTP-10628

- Fix improper setting of Application-ID in the Diameter header of an answer message whose E flag is set.

  The value should be that of the request in question. The fault caused it always to be 0.

  Own Id: OTP-10655

- Fix faulty handling of AVP length errors.

  An incorrect AVP length but no other errors caused an incoming request to fail.

  Own Id: OTP-10693

### 1.18 diameter 1.3.1

#### Known Bugs and Problems

- Fix function clause resulting from use of an eval callback.

  Own Id: OTP-10685

### 1.19 diameter 1.3

#### Fixed Bugs and Malfunctions

- Fix faulty handling of Origin-State-Id and faulty config values.

  The former was expected in a list despite the documentation requiring (correctly) an integer. A bare value for a list-valued capability was not handled.

  Own Id: OTP-10440

- Fix timing of up/down events.

  Previously, a call to diameter:call/4 following a peer_up callback might incorrectly return {error, no_connection}, depending on timing. Both events now follow the corresponding callbacks.

  Own Id: OTP-10459

- Make diameter:service_info/2 usable in peer_up, peer_down and pick_peer callbacks.

  Except for in pick_peer when {call_mutates_state, false}, it would previously hang indefinitely.

  Own Id: OTP-10460

- Verify that End-to-End and Hop-by-Hop Identifiers in an incoming CEA/DPA match those sent in the corresponding CER/DPR.

  The values were previously ignored. Answers whose identifiers do not match are handled as unexpected.

  Own Id: OTP-10565

- Fix formatting problems in PDF documentation.

  In particular, text corresponding to links in HTML was omitted in preformatted blocks. There are still issues with indentation but this is not diameter-specific.

  Own Id: OTP-10583

#### Improvements and New Features

- Let prepare_request, prepare_retransmit and handle_request callbacks return a function to be invoked on outgoing messages after encode.

  This allows encoded messages to be logged for example.

  Own Id: OTP-10441

- Add service_opt() 'restrict_connections' to allow multiple transport connections with the same peer.

  Own Id: OTP-10443

- Add service_opt() 'sequence' to allow the masking of a constant onto the topmost bits of End-to-End and Hop-by-Hop identifiers.

  This allows the same service on different nodes to use distinct values in outgoing request messages.

  Own Id: OTP-10445

- Add diameter:service_info(PeerRef) to return the transport_ref() and transport_opt() list of the corresponding transport.

  This allows easy access to these from diameter_app callbacks that only get peer_ref() as an argument.

  Own Id: OTP-10470

- Add reference pages diameter_codec(3) and diameter_make(3).

  Own Id: OTP-10471

- Add events for service start and stop.

  Own Id: OTP-10492

- Add transport_opt() 'disconnect_cb' to make the sending of DPR configurable.

  Whether or not DPR should be sent at application stop, service stop or transport removal is determined by the value returned by the callback, as is the Disconnect-Cause and timeout if DPA is not received.

  Own Id: OTP-10493

- Add transport_opt() 'capx_timeout' for the timeout associated with non-reception of CER/CEA.

  Own Id: OTP-10554

- Allow a handle_request callback to return a #diameter_packet{}.

  This allows an answer to set transport_data and header fields.

  Own Id: OTP-10566

- Update documentation for RFC 6733.

  RFC 3588 is now obsolete.

  Own Id: OTP-10568

### 1.20 diameter 1.2

#### Fixed Bugs and Malfunctions

- Fix broken Result-Code setting and Destination-Host/Realm extraction.

  Result-Code was assumed to have arity 1 when setting this value in an answer to a request containing AVP decode errors. Destination-Host/Realm were only correctly extracted from messages in the common application.

  Own Id: OTP-10202

- Handle insufficient capabilities configuration more gracefully.

  A transport that does not have sufficient capabilities configuration in order to encode CER/CEA will now emit an error report noting the configuration error and exit instead of failing. The error is not detected at diameter:add_transport/2 since there is no requirement that a service be configured before its transports.

  Own Id: OTP-10203

- Ensure a failing peer_up/down callback does not affect transport connections to other peers.

  Such a failure would previously have taken down all of a service's connections.

  Own Id: OTP-10215

#### Improvements and New Features

- Statistics related to Diameter messages can be retrieved using diameter:service_info/2.

  Both Diameter and socket-level statistics are available, for both incoming and outgoing messages.

  Own Id: OTP-9608

- Allow multiple transport_module/config to diameter:add_transport/2.

  Multiple values are attempted in sequence until one results in an established connection. This provides a way for a connecting transport to specify configuration in order of preference. (For example, SCTP before TCP.)

  Own Id: OTP-9885

- Add events for state transitions in the RFC 3539 watchdog state machine.

  The watchdog state is also available through diameter:service_info/2.

  Own Id: OTP-10212

- Add diameter:service_info(SvcName, connections).

  This provides an alternative to diameter:service_info(SvcName, transport) that presents information per established connection instead of per transport reference.

  Own Id: OTP-10213

- Assorted documentation corrections/improvements.

  Own Id: OTP-10216

### 1.21 diameter 1.1

#### Fixed Bugs and Malfunctions

- Fix fault in sending of 'closed' events.

  The fault made it possible for the 'closed' event not to be sent following a failed capabilities exchange.

  Own Id: OTP-9824

- Fix faulty diameterc -name/-prefix.

  A minor blunder when introducing the new dictionary parser in diameter-1.0 broke these options.

  Own Id: OTP-9826

### 1.22 diameter 1.0

#### Fixed Bugs and Malfunctions

- Fix faulty cleanup after diameter:remove_transport/2.

  Removing a transport removed the configuration but did not prevent the transport process from being restarted.

  Own Id: OTP-9756

#### Improvements and New Features

- Add support for TLS over TCP.

  RFC 3588 requires that a Diameter server support TLS. In practice this seems to mean TLS over SCTP since there are limitations with running over SCTP: see RFC 6083 (DTLS over SCTP), which is a response to RFC 3436 (TLS over SCTP). The current RFC 3588 draft acknowledges this by equating TLS with TLS/TCP and DTLS/SCTP.

  TLS handshaking can take place either following a CER/CEA that negotiates TLS using the Inband-Security-Id AVP (the method documented in RFC 3588) or immediately following connection establishment (the method added to the current draft).

  Own Id: OTP-9605

- Improvements to the dictionary parser.

  The dictionary parser now emits useful error messages in case of faults in the input file, also identifying the line number at which the fault was detected. There are semantic checks that were missing in the previous parser, a fault in the interpretation of vendor id's in combination with @inherits has been fixed and @end can be used to terminate parsing explicitly instead of always parsing to end of file.

  Own Id: OTP-9639

- Improve dictionary reusability.

  Reusing a dictionary just to get a different generated module name or prefix previously required taking a copy of the source, which may consist of several files if inheritance is used, just to edit a couple of lines which don't affect the semantics of the Diameter application being defined. Options --name, --prefix and --inherits have been added to diameterc to allow corresponding values to be set at compile time.

  Own Id: OTP-9641

- Add capabilities_cb transport option.

  Its value is a function that's applied to the transport reference and capabilities record after capabilities exchange. If a callback returns anything but 'ok' then the connection is closed. In the case of an incoming CER, the callback can return a result code with which to answer. Multiple callbacks can be specified and are applied until either all return 'ok' or one doesn't.

  This provides a way to reject a peer connection.

  Own Id: OTP-9654

- Add @codecs to dictionary format.

  The semantics are similar to @custom_types but results in codec functions of the form TypeName(encode|decode, AvpName, Data) rather than AvpName(encode|decode, TypeName, Data). That is, the role of the AVP name and Diameter type name are reversed. This eliminates the need for exporting one function for each AVP sharing a common specialized encode/decode.

  Own Id: OTP-9708 Aux Id: OTP-9639

- Add #diameter_callback{} for more flexible callback configuration.

  The record allows individual functions to be configured for each of the diameter_app(3) callbacks, as well as a default callback.

  Own Id: OTP-9777

### 1.23 diameter 0.10

#### Fixed Bugs and Malfunctions

- Handle #sctp_paddr_change and #sctp_pdapi_event from gen_sctp.

  The events are enabled by default but diameter_sctp neither disabled nor dealt with them. Reception of such an event caused a transport process to crash.

  Own Id: OTP-9538

- Fix header folding bug.

  A prepare_request callback from diameter can return a diameter_header record in order to set values in the header of an outgoing request. A fault in diameter_lib:fold_tuple/3 caused the subsequent encode of the outgoing request to fail.

  Own Id: OTP-9577

- Fix bugs in sending of answer-message replies.

  3001 (DIAMETER_COMMAND_UNSUPPORTED) was not sent since the decode placed the AVP list in the wrong field of the diameter_packet, causing the subsequent encode to fail. Session-Id was also set improperly, causing encode to fail even in this case.

  Own Id: OTP-9578

- Fix improper use of error_logger:info_report/2.

  Function doesn't take a format string and arguments as it was called. Instead use error_logger:info_report/1 and use the same report format as used for warning and error reports.

  Own Id: OTP-9579

- Fix and clarify semantics of peer filters.

  An eval filter returning a non-true value caused the call process to fail and the doc was vague on how an exception was treated. Clarify that the non-tuple host/realm filters assume messages of a certain form.

  Own Id: OTP-9580

- Fix and clarify relay behaviour.

  Implicit filtering of the sending peer in relaying a request could cause loop detection to be preempted in a manner not specified by RFC3588. Reply with 3002 (DIAMETER_UNABLE_TO_DELIVER) on anything but an answer to a relayed request.

  Own Id: OTP-9583

#### Improvements and New Features

- @id required in dictionary files only when @messages is specified.

  @id defines an application identifier and this is used only when sending or receiving messages. A dictionary can define only AVP's however, to be included by other dictionaries using @inherits, in which case it makes no sense to require @id.

  Note that message definitions are not inherited with @inherits, only AVP's

  Own Id: OTP-9467

- Allow @enum when AVP is defined in an inherited dictionary.

  3GPP standards (for one) extend the values allowed for RFC 3588 AVP's of type Enumerated. Previously, extending an AVP was only possible by completely redefining the AVP.

  Own Id: OTP-9469

- Migrate testsuites to pure common test and add both suites and testcases.

  Own Id: OTP-9553

- Requests of arbitrary form.

  diameter:call/4 can be passed anything, as long as the subsequent prepare_request callback returns a term that can be encoded.

  Own Id: OTP-9581

### 1.24 diameter 0.9

Initial release of the diameter application.

Known issues or limitations:

- Some agent-related functionality is not entirely complete. In particular, support for proxy agents, that advertise specific Diameter applications but otherwise relay messages in much the same way as relay agents (for which a handle_request callback can return a relay tuple), will be completed in an upcoming release. There may also be more explicit support for redirect agents, although redirect behaviour can be implemented with the current functionality.

- There is some asymmetry in the treatment of messages sent as diameter_header/avp records and those sent in the "normal" fashion, and not all of this is documented. This is related to the previous point since this form of sending a message was introduced specifically to handle relay agent behaviour using the same callback interface as for client/server behaviour.

- The User's Guide is currently quite thin. The introductory chapter followed by the examples (in the application examples subdirectory) may be sufficient for those having some familiarity with the Diameter protocol but the intention is to provide more introductory text. The reference documentation is quite complete, although some points could likely be expanded upon.

- The function diameter:service_info/2 can be used to retrieve information about a started service (statistics, information about connected peers, etc) but this is not yet documented and both the input and output may change in the next release.

See Standards Compliance for standards-related issues.