User's Guide
Reference Manual
Release Notes
PDF
Top

ASN.1
User's Guide
Version 4.0.1

Expand All
Contract All

Chapters

- Introduction
  - Top of chapter
  - Scope
  - Prerequisites
- ASN.1
  - Top of chapter
  - Introduction
- Getting Started
  - Top of chapter
  - Example
  - ASN.1 Application User Interface
  - Multi-File Compilation
  - Remark about Tags
  - ASN.1 Types
  - Naming of Records in .hrl Files
  - ASN.1 Values
  - Macros
  - ASN.1 Information Objects (X.681)
  - Parameterization (X.683)
- Specialized Decodes
  - Top of chapter
  - Exclusive Decode
  - Selective Decode
  - Performance

# 3 Getting Started

### 3.1 Example

The following example demonstrates the basic functionality used to run the Erlang ASN.1 compiler.

Create a file named People.asn containing the following:

    People DEFINITIONS AUTOMATIC TAGS ::=
    BEGIN
      Person ::= SEQUENCE {
        name PrintableString,
        location INTEGER {home(0),field(1),roving(2)},
        age INTEGER OPTIONAL
      }
    END

This file must be compiled before it can be used. The ASN.1 compiler checks that the syntax is correct and that the text represents proper ASN.1 code before generating an abstract syntax tree. The code-generator then uses the abstract syntax tree to generate code.

The generated Erlang files are placed in the current directory or in the directory specified with option {outdir,Dir}.

The following shows how the compiler can be called from the Erlang shell:

    1> asn1ct:compile("People", [ber]).
    ok
    2>

Option verbose can be added to get information about the generated files:

    2> asn1ct:compile("People", [ber,verbose]).
    Erlang ASN.1 compiling "People.asn"
    --{generated,"People.asn1db"}--
    --{generated,"People.hrl"}--
    --{generated,"People.erl"}--
    ok
    3>

ASN.1 module People is now accepted and the abstract syntax tree is saved in file People.asn1db. The generated Erlang code is compiled using the Erlang compiler and loaded into the Erlang runtime system. There is now an API for encode/2 and decode/2 in module People, which is called like:
'People':encode(<Type name>, <Value>)
or
'People':decode(<Type name>, <Value>)

Assume that there is a network application that receives instances of the ASN.1 defined type Person, modifies, and sends them back again:

    receive
       {Port,{data,Bytes}} ->
           case 'People':decode('Person',Bytes) of
               {ok,P} ->
                   {ok,Answer} = 'People':encode('Person',mk_answer(P)),
                   Port ! {self(),{command,Answer}};
               {error,Reason} ->
                   exit({error,Reason})
           end
        end,

In this example, a series of bytes is received from an external source and the bytes are then decoded into a valid Erlang term. This was achieved with the call 'People':decode('Person',Bytes), which returned an Erlang value of the ASN.1 type Person. Then an answer was constructed and encoded using 'People':encode('Person',Answer), which takes an instance of a defined ASN.1 type and transforms it to a binary according to the BER or PER encoding rules.

The encoder and decoder can also be run from the shell:

    2> Rockstar = {'Person',"Some Name",roving,50}.
    {'Person',"Some Name",roving,50}
    3> {ok,Bin} = 'People':encode('Person',Rockstar).
    {ok,<<243,17,19,9,83,111,109,101,32,78,97,109,101,2,1,2,
          2,1,50>>}
    4> {ok,Person} = 'People':decode('Person',Bin).
    {ok,{'Person',"Some Name",roving,50}}
    5>

#### Module Dependencies

It is common that ASN.1 modules import defined types, values, and other entities from another ASN.1 module.

Earlier versions of the ASN.1 compiler required that modules that were imported from had to be compiled before the module that imported. This caused problems when ASN.1 modules had circular dependencies.

Referenced modules are now parsed when the compiler finds an entity that is imported. No code is generated for the referenced module. However, the compiled modules rely on that the referenced modules are also compiled.

### 3.2 ASN.1 Application User Interface

The ASN.1 application provides the following two separate user interfaces:

- The module asn1ct, which provides the compile-time functions (including the compiler)

- The module asn1rt_nif, which provides the runtime functions for the ASN.1 decoder for the BER back end

The reason for this division of the interfaces into compile-time and runtime is that only runtime modules (asn1rt*) need to be loaded in an embedded system.

#### Compile-Time Functions

The ASN.1 compiler can be started directly from the command line by the erlc program. This is convenient when compiling many ASN.1 files from the command line or when using Makefiles. Some examples of how the erlc command can be used to start the ASN.1 compiler:

    erlc Person.asn
    erlc -bper Person.asn
    erlc -bber ../Example.asn
    erlc -o ../asnfiles -I ../asnfiles -I /usr/local/standards/asn1 Person.asn

Useful options for the ASN.1 compiler:

-b[ber | per | uper]

  Choice of encoding rules. If omitted, ber is the default.

-o OutDirectory

  Where to put the generated files. Default is the current directory.

-I IncludeDir

  Where to search for .asn1db files and ASN.1 source specs to resolve references to other modules. This option can be repeated many times if there are several places to search in. The compiler searches the current directory first.

+der

  DER encoding rule. Only when using option -ber.

+asn1config

  This functionality works together with option ber. It enables the specialized decodes, see Section Specialized Decode.

+undec_rest

  A buffer that holds a message being decoded can also have trailing bytes. If those trailing bytes are important, they can be returned along with the decoded value by compiling the ASN.1 specification with option +undec_rest. The return value from the decoder is {ok,Value,Rest} where Rest is a binary containing the trailing bytes.

+'Any Erlc Option'

  Any option can be added to the Erlang compiler when compiling the generated Erlang files. Any option unrecognized by the ASN.1 compiler is passed to the Erlang compiler.

For a complete description of erlc, see ERTS Reference Manual.

The compiler and other compile-time functions can also be started from the Erlang shell. Here follows a brief description of the primary functions. For a complete description of each function, see module asn1ct in the ASN.1 Reference Manual.

The compiler is started by asn1ct:compile/1 with default options, or asn1ct:compile/2 if explicit options are given.

Example:

    asn1ct:compile("H323-MESSAGES.asn1").

This equals:

    asn1ct:compile("H323-MESSAGES.asn1",[ber]).

If PER encoding is wanted:

    asn1ct:compile("H323-MESSAGES.asn1",[per]).

The generic encode and decode functions can be called as follows:

    'H323-MESSAGES':encode('SomeChoiceType',{call,<<"octetstring">>}).
    'H323-MESSAGES':decode('SomeChoiceType',Bytes).

#### Runtime Functions

When an ASN.1 specification is compiled with option ber, the asn1rt_nif module and the NIF library in asn1/priv_dir are needed at runtime.

By calling function info/0 in a generated module, you get information about which compiler options were used.

#### Errors

Errors detected at compile-time are displayed on the screen together with line numbers indicating where in the source file the respective error was detected. If no errors are found, an Erlang ASN.1 module is created.

The runtime encoders and decoders execute within a catch and return {ok, Data} or {error, {asn1, Description}} where Description is an Erlang term describing the error.

### 3.3 Multi-File Compilation

There are various reasons for using multi-file compilation:

- To choose the name for the generated module, for example, because you need to compile the same specs for different encoding rules.
- You want only one resulting module.

Specify which ASN.1 specs to compile in a module with extension .set.asn. Choose a module name and provide the names of the ASN.1 specs. For example, if you have the specs File1.asn, File2.asn, and File3.asn, your module MyModule.set.asn looks as follows:

    File1.asn
    File2.asn
    File3.asn

If you compile with the following, the result is one merged module MyModule.erl with the generated code from the three ASN.1 specs:

    ~> erlc MyModule.set.asn

### 3.4 Remark about Tags

Tags used to be important for all users of ASN.1, because it was necessary to add tags manually to certain constructs in order for the ASN.1 specification to be valid. Example of an old-style specification:

    Tags DEFINITIONS ::=
    BEGIN
      Afters ::= CHOICE { cheese [0] IA5String,
                          dessert [1] IA5String }
    END

Without the tags (the numbers in square brackets) the ASN.1 compiler refused to compile the file.

In 1994 the global tagging mode AUTOMATIC TAGS was introduced. By putting AUTOMATIC TAGS in the module header, the ASN.1 compiler automatically adds tags when needed. The following is the same specification in AUTOMATIC TAGS mode:

    Tags DEFINITIONS AUTOMATIC TAGS ::=
    BEGIN
      Afters ::= CHOICE { cheese IA5String,
                          dessert IA5String }
    END

Tags are not mentioned any more in this User's Guide.

### 3.5 ASN.1 Types

This section describes the ASN.1 types including their functionality, purpose, and how values are assigned in Erlang.

ASN.1 has both primitive and constructed types:

Primitive Types | Constructed Types
BOOLEAN | SEQUENCE
INTEGER | SET
REAL | CHOICE
NULL | SET OF and SEQUENCE OF
ENUMERATED | ANY
BIT STRING | ANY DEFINED BY
OCTET STRING | EXTERNAL
Character Strings | EMBEDDED PDV
OBJECT IDENTIFIER | CHARACTER STRING
Object Descriptor |
TIME Types |

Table 3.1: Supported ASN.1 Types
Note

The values of each ASN.1 type have their own representation in Erlang, as described in the following sections. Users must provide these values for encoding according to the representation, as shown in the following example:

    Operational ::= BOOLEAN --ASN.1 definition

In Erlang code it can look as follows:

    Val = true,
    {ok,Bytes} = MyModule:encode('Operational', Val),

#### BOOLEAN

Booleans in ASN.1 express values that can be either TRUE or FALSE. The meanings assigned to TRUE and FALSE are outside the scope of this text.

In ASN.1 it is possible to have:

    Operational ::= BOOLEAN

Assigning a value to type Operational in Erlang is possible by using the following Erlang code:

    Myvar1 = true,

Thus, in Erlang the atoms true and false are used to encode a boolean value.

#### INTEGER

ASN.1 itself specifies indefinitely large integers. Erlang systems with version 4.3 and higher support very large integers, in practice indefinitely large integers.

The concept of subtyping can be applied to integers and to other ASN.1 types. The details of subtyping are not explained here; for more information, see X.680. Various syntaxes are allowed when defining a type as an integer:

    T1 ::= INTEGER
    T2 ::= INTEGER (-2..7)
    T3 ::= INTEGER (0..MAX)
    T4 ::= INTEGER (0<..MAX)
    T5 ::= INTEGER (MIN<..-99)
    T6 ::= INTEGER {red(0),blue(1),white(2)}

The Erlang representation of an ASN.1 INTEGER is an integer or an atom if a Named Number List (see T6 in the previous list) is specified.

The following is an example of Erlang code that assigns values for the types in the previous list:

    T1value = 0,
    T2value = 6,
    T6value1 = blue,
    T6value2 = 0,
    T6value3 = white

These Erlang variables are now bound to valid instances of ASN.1 defined types. This style of value can be passed directly to the encoder for transformation into a series of bytes.

The decoder returns an atom if the value corresponds to a symbol in the Named Number List.

#### REAL

The following ASN.1 type is used for real numbers:

    R1 ::= REAL

It is assigned a value in Erlang as follows:

    R1value1 = "2.14",
    R1value2 = {256,10,-2},

In the last line, notice that the tuple {256,10,-2} is the real number 2.56 in a special notation, which encodes faster than simply stating the number as "2.56". The arity three tuple is {Mantissa,Base,Exponent}, that is, Mantissa * Base^Exponent.

#### NULL

The type NULL is suitable where supply and recognition of a value is important but the actual value is not.

    Notype ::= NULL

This type is assigned in Erlang as follows:

    N1 = 'NULL',

The actual value is the quoted atom 'NULL'.

#### ENUMERATED

The type ENUMERATED can be used when the value you want to describe can only take one of a set of predefined values. Example:

    DaysOfTheWeek ::= ENUMERATED {
        sunday(1),monday(2),tuesday(3),
        wednesday(4),thursday(5),friday(6),saturday(7) }

For example, to assign a weekday value in Erlang, use the same atom as in the Enumerations of the type definition:

    Day1 = saturday,

The enumerated type is similar to an integer type, when defined with a set of predefined values. The difference is that an enumerated type can only have specified values, whereas an integer can have any value.

#### BIT STRING

The type BIT STRING can be used to model information that is made up of arbitrary length series of bits. It is intended to be used for selection of flags, not for binary files.

In ASN.1, BIT STRING definitions can look as follows:

    Bits1 ::= BIT STRING
    Bits2 ::= BIT STRING {foo(0),bar(1),gnu(2),gnome(3),punk(14)}

The following two notations are available for representation of BIT STRING values in Erlang and as input to the encode functions:

- A bitstring. By default, a BIT STRING with no symbolic names is decoded to an Erlang bitstring.
- A list of atoms corresponding to atoms in the NamedBitList in the BIT STRING definition. A BIT STRING with symbolic names is always decoded to the format shown in the following example:

    Bits1Val1 = <<0:1,1:1,0:1,1:1,1:1>>,
    Bits2Val1 = [gnu,punk],
    Bits2Val2 = <<2#1110:4>>,
    Bits2Val3 = [bar,gnu,gnome],

Bits2Val2 and Bits2Val3 denote the same value.

Bits2Val1 is assigned symbolic values. The assignment means that the bits corresponding to gnu and punk, that is, bits 2 and 14 are set to 1, and the rest are set to 0. The symbolic values are shown as a list of values. If a named value, which is not specified in the type definition, is shown, a runtime error occurs.

BIT STRINGs can also be subtyped with, for example, a SIZE specification:

    Bits3 ::= BIT STRING (SIZE(0..31))

This means that no bit higher than 31 can be set.

#### Deprecated Representations for BIT STRING

In addition to the representations described earlier, the following deprecated representations are available if the specification has been compiled with option legacy_erlang_types:

- Aa a list of binary digits (0 or 1). This format is accepted as input to the encode functions, and a BIT STRING is decoded to this format if option legacy_bit_string is given.
- As {Unused,Binary} where Unused denotes how many trailing zero-bits 0-7 that are unused in the least significant byte in Binary. This format is accepted as input to the encode functions, and a BIT STRING is decoded to this format if compact_bit_string has been given.
- As a hexadecimal number (or an integer). Avoid this as it is easy to misinterpret a BIT STRING value in this format.

#### OCTET STRING

OCTET STRING is the simplest of all ASN.1 types. OCTET STRING only moves or transfers, for example, binary files or other unstructured information complying with two rules: the bytes consist of octets and encoding is not required.

It is possible to have the following ASN.1 type definitions:

    O1 ::= OCTET STRING
    O2 ::= OCTET STRING (SIZE(28))

With the following example assignments in Erlang:

    O1Val = <<17,13,19,20,0,0,255,254>>,
    O2Val = <<"must be exactly 28 chars....">>,

By default, an OCTET STRING is always represented as an Erlang binary. If the specification has been compiled with option legacy_erlang_types, the encode functions accept both lists and binaries, and the decode functions decode an OCTET STRING to a list.

#### Character Strings

ASN.1 supports a wide variety of character sets. The main difference between an OCTET STRING and a character string is that the OCTET STRING has no imposed semantics on the bytes delivered.

However, when using, for example, IA5String (which closely resembles ASCII), byte 65 (in decimal notation) means character 'A'.

For example, if a defined type is to be a VideotexString and an octet is received with the unsigned integer value X, the octet is to be interpreted as specified in standard ITU-T T.100, T.101.

The ASN.1 to Erlang compiler does not determine the correct interpretation of each BER string octet value with different character strings. The application is responsible for interpretation of octets. Therefore, from the BER string point of view, octets are very similar to character strings and are compiled in the same way.

When PER is used, there is a significant difference in the encoding scheme between OCTET STRINGs and other strings. The constraints specified for a type are especially important for PER, where they affect the encoding.

Examples:

    Digs ::= NumericString (SIZE(1..3))
    TextFile ::= IA5String (SIZE(0..64000))

The corresponding Erlang assignments:

    DigsVal1 = "456",
    DigsVal2 = "123",
    TextFileVal1 = "abc...xyz...",
    TextFileVal2 = [88,76,55,44,99,121 .......... a lot of characters here ....]

The Erlang representation for "BMPString" and "UniversalString" is either a list of ASCII values or a list of quadruples. The quadruple representation associates to the Unicode standard representation of characters. The ASCII characters are all represented by quadruples beginning with three zeros like {0,0,0,65} for character 'A'. When decoding a value for these strings, the result is a list of quadruples, or integers when the value is an ASCII character.

The following example shows how it works. Assume the following specification is in file PrimStrings.asn1:

    PrimStrings DEFINITIONS AUTOMATIC TAGS ::=
    BEGIN
       BMP ::= BMPString
    END

Encoding and decoding some strings:

    1> asn1ct:compile('PrimStrings', [ber]).
    ok
    2> {ok,Bytes1} = 'PrimStrings':encode('BMP', [{0,0,53,53},{0,0,45,56}]).
    {ok,<<30,4,53,54,45,56>>}
    3> 'PrimStrings':decode('BMP', Bytes1).
    {ok,[{0,0,53,53},{0,0,45,56}]}
    4> {ok,Bytes2} = 'PrimStrings':encode('BMP', [{0,0,53,53},{0,0,0,65}]).
    {ok,<<30,4,53,53,0,65>>}
    5> 'PrimStrings':decode('BMP', Bytes2).
    {ok,[{0,0,53,53},65]}
    6> {ok,Bytes3} = 'PrimStrings':encode('BMP', "BMP string").
    {ok,<<30,20,0,66,0,77,0,80,0,32,0,115,0,116,0,114,0,105,0,110,0,103>>}
    7> 'PrimStrings':decode('BMP', Bytes3).
    {ok,"BMP string"}

Type UTF8String is represented as a UTF-8 encoded binary in Erlang. Such binaries can be created directly using the binary syntax or by converting from a list of Unicode code points using function unicode:characters_to_binary/1.

The following shows examples of how UTF-8 encoded binaries can be created and manipulated:

    1> Gs = "Мой маленький Гном".
    [1052,1086,1081,32,1084,1072,1083,1077,1085,1100,1082,1080,
     1081,32,1043,1085,1086,1084]
    2> Gbin = unicode:characters_to_binary(Gs).
    <<208,156,208,190,208,185,32,208,188,208,176,208,187,208,
      181,208,189,209,140,208,186,208,184,208,185,32,208,147,
      208,...>>
    3> Gbin = <<"Мой маленький Гном"/utf8>>.
    <<208,156,208,190,208,185,32,208,188,208,176,208,187,208,
      181,208,189,209,140,208,186,208,184,208,185,32,208,147,
      208,...>>
    4> Gs = unicode:characters_to_list(Gbin).
    [1052,1086,1081,32,1084,1072,1083,1077,1085,1100,1082,1080,
     1081,32,1043,1085,1086,1084]

For details, see the unicode module in stdlib.

In the following example, this ASN.1 specification is used:

    UTF DEFINITIONS AUTOMATIC TAGS ::=
    BEGIN
       UTF ::= UTF8String
    END

Encoding and decoding a string with Unicode characters:

    5> asn1ct:compile('UTF', [ber]).
    ok
    6> {ok,Bytes1} = 'UTF':encode('UTF', <<"Гном"/utf8>>).
    {ok,<<12,8,208,147,208,189,208,190,208,188>>}
    7> {ok,Bin1} = 'UTF':decode('UTF', Bytes1).
    {ok,<<208,147,208,189,208,190,208,188>>}
    8> io:format("~ts\n", [Bin1]).
    Гном
    ok
    9> unicode:characters_to_list(Bin1).
    [1043,1085,1086,1084]

#### OBJECT IDENTIFIER

The type OBJECT IDENTIFIER is used whenever a unique identity is required. An ASN.1 module, a transfer syntax, and so on, is identified with an OBJECT IDENTIFIER. Assume the following example:

    Oid ::= OBJECT IDENTIFIER

Therefore, the following example is a valid Erlang instance of type 'Oid':

    OidVal1 = {1,2,55},

The OBJECT IDENTIFIER value is simply a tuple with the consecutive values, which must be integers.

The first value is limited to the values 0, 1, or 2. The second value must be in the range 0..39 when the first value is 0 or 1.

The OBJECT IDENTIFIER is an important type and it is widely used within different standards to identify various objects uniquely. Dubuisson: ASN.1 - Communication Between Heterogeneous Systems includes an easy-to-understand description of the use of OBJECT IDENTIFIER.

#### Object Descriptor

Values of this type can be assigned a value as an ordinary string as follows:

          "This is the value of an Object descriptor"

#### TIME Types

Two time types are defined within ASN.1: Generalized Time and Universal Time Coordinated (UTC). Both are assigned a value as an ordinary string within double quotes, for example, "19820102070533.8".

For DER encoding, the compiler does not check the validity of the time values. The DER requirements upon those strings are regarded as a matter for the application to fulfill.

#### SEQUENCE

The structured types of ASN.1 are constructed from other types in a manner similar to the concepts of array and struct in C.

A SEQUENCE in ASN.1 is comparable with a struct in C and a record in Erlang. A SEQUENCE can be defined as follows:

    Pdu ::= SEQUENCE {
       a INTEGER,
       b REAL,
       c OBJECT IDENTIFIER,
       d NULL }

This is a 4-component structure called Pdu. The record format is the major format for representation of SEQUENCE in Erlang. For each SEQUENCE and SET in an ASN.1 module an Erlang record declaration is generated. For Pdu, a record like the following is defined:

    -record('Pdu',{a, b, c, d}).

The record declarations for a module M are placed in a separate M.hrl file.

Values can be assigned in Erlang as follows:

    MyPdu = #'Pdu'{a=22,b=77.99,c={0,1,2,3,4},d='NULL'}.

The decode functions return a record as result when decoding a SEQUENCE or a SET.

A SEQUENCE and a SET can contain a component with a DEFAULT keyword followed by the actual value, which is the default value. The DEFAULT keyword means that the application doing the encoding can omit encoding of the value, which results in fewer bytes to send to the receiving application.

An application can use the atom asn1_DEFAULT to indicate that the encoding is to be omitted for that position in the SEQUENCE.

Depending on the encoding rules, the encoder can also compare the given value to the default value and automatically omit the encoding if the values are equal. How much effort the encoder makes to compare the values depends on the encoding rules. The DER encoding rules forbid encoding a value equal to the default value, so it has a more thorough and time-consuming comparison than the encoders for the other encoding rules.

In the following example, this ASN.1 specification is used:

    File DEFINITIONS AUTOMATIC TAGS ::=
    BEGIN
    Seq1 ::= SEQUENCE {
        a INTEGER DEFAULT 1,
        b Seq2 DEFAULT {aa TRUE, bb 15}
    }

    Seq2 ::= SEQUENCE {
        aa BOOLEAN,
        bb INTEGER
    }

    Seq3 ::= SEQUENCE {
        bs BIT STRING {a(0), b(1), c(2)} DEFAULT {a, c}
    }
    END

Example where the BER encoder is able to omit encoding of the default values:

    1> asn1ct:compile('File', [ber]).
    ok
    2> 'File':encode('Seq1', {'Seq1',asn1_DEFAULT,asn1_DEFAULT}).
    {ok,<<48,0>>}
    3> 'File':encode('Seq1', {'Seq1',1,{'Seq2',true,15}}).
    {ok,<<48,0>>}

Example with a named BIT STRING where the BER encoder does not omit the encoding:

    4> 'File':encode('Seq3', {'Seq3',asn1_DEFAULT).
    {ok,<<48,0>>}
    5> 'File':encode('Seq3', {'Seq3',<<16#101:3>>).
    {ok,<<48,4,128,2,5,160>>}

The DER encoder omits the encoding for the same BIT STRING:

    6> asn1ct:compile('File', [ber,der]).
    ok
    7> 'File':encode('Seq3', {'Seq3',asn1_DEFAULT).
    {ok,<<48,0>>}
    8> 'File':encode('Seq3', {'Seq3',<<16#101:3>>).
    {ok,<<48,0>>}

#### SET

In Erlang, the SET type is used exactly as SEQUENCE. Notice that if BER or DER encoding rules are used, decoding a SET is slower than decoding a SEQUENCE because the components must be sorted.

#### Extensibility for SEQUENCE and SET

When a SEQUENCE or SET contains an extension marker and extension components as the following, the type can get more components in newer versions of the ASN.1 spec:

    SExt ::= SEQUENCE {
               a INTEGER,
               ...,
               b BOOLEAN }

In this case it has got a new component b. Thus, incoming messages that are decoded can have more or fever components than this one.

The component b is treated as an original component when encoding a message. In this case, as it is not an optional element, it must be encoded.

During decoding, the b field of the record gets the decoded value of the b component, if present, otherwise the value asn1_NOVALUE.

#### CHOICE

The type CHOICE is a space saver and is similar to the concept of a 'union' in C.

Assume the following:

    SomeModuleName DEFINITIONS AUTOMATIC TAGS ::=
    BEGIN
    T ::= CHOICE {
            x REAL,
            y INTEGER,
            z OBJECT IDENTIFIER }
    END

It is then possible to assign values as follows:

    TVal1 = {y,17},
    TVal2 = {z,{0,1,2}},

A CHOICE value is always represented as the tuple {ChoiceAlternative, Val} where ChoiceAlternative is an atom denoting the selected choice alternative.

#### Extensible CHOICE

When a CHOICE contains an extension marker and the decoder detects an unknown alternative of the CHOICE, the value is represented as follows:

    {asn1_ExtAlt, BytesForOpenType}

Here BytesForOpenType is a list of bytes constituting the encoding of the "unknown" CHOICE alternative.

#### SET OF and SEQUENCE OF

The types SET OF and SEQUENCE OF correspond to the concept of an array in several programming languages. The Erlang syntax for both types is straightforward, for example:

    Arr1 ::= SET SIZE (5) OF INTEGER (4..9)
    Arr2 ::= SEQUENCE OF OCTET STRING

In Erlang the following can apply:

    Arr1Val = [4,5,6,7,8],
    Arr2Val = ["abc",[14,34,54],"Octets"],

Notice that the definition of type SET OF implies that the order of the components is undefined, but in practice there is no difference between SET OF and SEQUENCE OF. The ASN.1 compiler for Erlang does not randomize the order of the SET OF components before encoding.

However, for a value of type SET OF, the DER encoding format requires the elements to be sent in ascending order of their encoding, which implies an expensive sorting procedure in runtime. Therefore it is recommended to use SEQUENCE OF instead of SET OF if possible.

#### ANY and ANY DEFINED BY

The types ANY and ANY DEFINED BY have been removed from the standard since 1994. It is recommended not to use these types any more. They can, however, exist in some old ASN.1 modules. The idea with this type was to leave a "hole" in a definition where it was possible to put unspecified data of any kind, even non-ASN.1 data.

A value of this type is encoded as an open type.

Instead of ANY and ANY DEFINED BY, it is recommended to use information object class, table constraints, and parameterization. In particular the construct TYPE-IDENTIFIER.@Type accomplish the same as the deprecated ANY.

See also Information object.

#### EXTERNAL, EMBEDDED PDV, and CHARACTER STRING

The types EXTERNAL, EMBEDDED PDV, and CHARACTER STRING are used in presentation layer negotiation. They are encoded according to their associated type, see X.680.

The type EXTERNAL had a slightly different associated type before 1994. X.691 states that encoding must follow the older associated type. So, generated encode/decode functions convert values of the newer format to the older format before encoding. This implies that it is allowed to use EXTERNAL type values of either format for encoding. Decoded values are always returned in the newer format.

#### Embedded Named Types

The structured types previously described can have other named types as their components. The general syntax to assign a value to component C of a named ASN.1 type T in Erlang is the record syntax #'T'{'C'=Value}. Here Value can be a value of yet another type T2, for example:

    EmbeddedExample DEFINITIONS AUTOMATIC TAGS ::=
    BEGIN
    B ::= SEQUENCE {
            a Arr1,
            b T }

    Arr1 ::= SET SIZE (5) OF INTEGER (4..9)

    T ::= CHOICE {
            x REAL,
            y INTEGER,
            z OBJECT IDENTIFIER }
            END

SEQUENCE b can be encoded as follows in Erlang:

    1> 'EmbeddedExample':encode('B', {'B',[4,5,6,7,8],{x,"7.77"}}).
    {ok,<<5,56,0,8,3,55,55,55,46,69,45,50>>}

### 3.6 Naming of Records in .hrl Files

When an ASN.1 specification is compiled, all defined types of type SET or SEQUENCE result in a corresponding record in the generated .hrl file. This is because the values for SET and SEQUENCE are represented as records as mentioned earlier.

Some special cases of this functionality are presented in the next section.

#### Embedded Structured Types

In ASN.1 it is also possible to have components that are themselves structured types. For example, it is possible to have the following:

    Emb ::= SEQUENCE {
        a SEQUENCE OF OCTET STRING,
        b SET {
           a INTEGER,
           b INTEGER DEFAULT 66},
        c CHOICE {
           a INTEGER,
           b FooType } }

    FooType ::= [3] VisibleString

The following records are generated because of type Emb:

    -record('Emb,{a, b, c}).
    -record('Emb_b',{a, b = asn1_DEFAULT}). % the embedded SET type

Values of type Emb can be assigned as follows:

    V = #'Emb'{a=["qqqq",[1,2,255]],
               b = #'Emb_b'{a=99},
               c ={b,"Can you see this"}}.

For an embedded type of type SEQUENCE/SET in a SEQUENCE/SET, the record name is extended with an underscore and the component name. If the embedded structure is deeper with the SEQUENCE, SET, or CHOICE types in the line, each component name/alternative name is added to the record name.

Example:

    Seq ::= SEQUENCE{
        a CHOICE{
            b SEQUENCE {
               c  INTEGER
            }
        }
    }

This results in the following record:

    -record('Seq_a_b',{c}).

If the structured type has a component with an embedded SEQUENCE OF/SET OF which embedded type in turn is a SEQUENCE/SET, it gives a record with the SEQUENCE OF/SET OF addition as in the following example:

    Seq ::= SEQUENCE {
        a SEQUENCE OF SEQUENCE {
               b
                   }
        c SET OF SEQUENCE {
               d
                   }
    }

This results in the following records:

    -record('Seq_a_SEQOF'{b}).
    -record('Seq_c_SETOF'{d}).

A parameterized type is to be considered as an embedded type. Each time such a type is referenced, an instance of it is defined. Thus, in the following example a record with name 'Seq_b' is generated in the .hrl file and is used to hold values:

    Seq ::= SEQUENCE {
        b PType{INTEGER}
    }

    PType{T} ::= SEQUENCE{
        id T
    }

#### Recursive Types

Types that refer to themselves are called recursive types. Example:

    Rec ::= CHOICE {
         nothing NULL,
         something SEQUENCE {
              a INTEGER,
              b OCTET STRING,
              c Rec }}

This is allowed in ASN.1 and the ASN.1-to-Erlang compiler supports this recursive type. A value for this type is assigned in Erlang as follows:

    V = {something,#'Rec_something'{a = 77,
                                    b = "some octets here",
                                    c = {nothing,'NULL'}}}.

### 3.7 ASN.1 Values

Values can be assigned to an ASN.1 type within the ASN.1 code itself, as opposed to the actions in the previous section where a value was assigned to an ASN.1 type in Erlang. The full value syntax of ASN.1 is supported and X.680 describes in detail how to assign values in ASN.1. A short example:

    TT ::= SEQUENCE {
       a INTEGER,
       b SET OF OCTET STRING }

    tt TT ::= {a 77,b {"kalle","kula"}}

The value defined here can be used in several ways. It can, for example, be used as the value in some DEFAULT component:

    SS ::= SET {
        s OBJECT IDENTIFIER,
        val TT DEFAULT tt }

It can also be used from inside an Erlang program. If this ASN.1 code is defined in ASN.1 module Values, the ASN.1 value tt can be reached from Erlang as a function call to 'Values':tt() as in the following example:

    1> Val = 'Values':tt().
    {'TT',77,["kalle","kula"]}
    2> {ok,Bytes} = 'Values':encode('TT',Val).
    {ok,<<48,18,128,1,77,161,13,4,5,107,97,108,108,101,4,4,
          107,117,108,97>>}
    4> 'Values':decode('TT',Bytes).
    {ok,{'TT',77,["kalle","kula"]}}
    5>

This example shows that a function is generated by the compiler that returns a valid Erlang representation of the value, although the value is of a complex type.

Furthermore, a macro is generated for each value in the .hrl file. So, the defined value tt can also be extracted by ?tt in application code.

### 3.8 Macros

The type MACRO is not supported. It is no longer part of the ASN.1 standard.

### 3.9 ASN.1 Information Objects (X.681)

Information Object Classes, Information Objects, and Information Object Sets (in the following called classes, objects, and object sets, respectively) are defined in the standard definition X.681. Only a brief explanation is given here.

These constructs makes it possible to define open types, that is, values of that type can be of any ASN.1 type. Also, relationships can be defined between different types and values, as classes can hold types, values, objects, object sets, and other classes in their fields. A class can be defined in ASN.1 as follows:

    GENERAL-PROCEDURE ::= CLASS {
          &Message,
          &Reply               OPTIONAL,
          &Error               OPTIONAL,
          &id          PrintableString UNIQUE
    }
    WITH SYNTAX {
          NEW MESSAGE     &Message
          [REPLY           &Reply]
          [ERROR           &Error]
          ADDRESS          &id
    }

An object is an instance of a class. An object set is a set containing objects of a specified class. A definition can look as follows:

    object1 GENERAL-PROCEDURE ::= {
        NEW MESSAGE      PrintableString
        ADDRESS          "home"
    }

    object2 GENERAL-PROCEDURE ::= {
        NEW MESSAGE INTEGER
        ERROR INTEGER
        ADDRESS "remote"
    }

The object object1 is an instance of the class GENERAL-PROCEDURE and has one type field and one fixed type value field. The object object2 has also an optional field ERROR, which is a type field. The field ADDRESS is a UNIQUE field. Objects in an object set must have unique values in their UNIQUE field, as in GENERAL-PROCEDURES:

    GENERAL-PROCEDURES GENERAL-PROCEDURE ::= {
        object1 | object2}

You cannot encode a class, object, or object set, only refer to it when defining other ASN.1 entities. Typically you refer to a class as well as to object sets by table constraints and component relation constraints (X.682) in ASN.1 types, as in the following:

    StartMessage  ::= SEQUENCE {
        msgId  GENERAL-PROCEDURE.&id  ({GENERAL-PROCEDURES}),
        content GENERAL-PROCEDURE.&Message ({GENERAL-PROCEDURES}{@msgId}),
        }

In type StartMessage, the constraint following field content tells that in a value of type StartMessage the value in field content must come from the same object that is chosen by field msgId.

So, the value #'StartMessage'{msgId="home",content="Any Printable String"} is legal to encode as a StartMessage value. However, the value #'StartMessage'{msgId="remote", content="Some String"} is illegal as the constraint in StartMessage tells that when you have chosen a value from a specific object in object set GENERAL-PROCEDURES in field msgId, you must choose a value from that same object in the content field too. In this second case, it is to be any INTEGER value.

StartMessage can in field content be encoded with a value of any type that an object in object set GENERAL-PROCEDURES has in its NEW MESSAGE field. This field refers to a type field &Message in the class. Field msgId is always encoded as a PrintableString, as the field refers to a fixed type in the class.

In practice, object sets are usually declared to be extensible so that more objects can be added to the set later. Extensibility is indicated as follows:

    GENERAL-PROCEDURES GENERAL-PROCEDURE ::= {
        object1 | object2, ...}

When decoding a type that uses an extensible set constraint, it is always possible that the value in field UNIQUE is unknown (that is, the type has been encoded with a later version of the ASN.1 specification). The unencoded data is then returned wrapped in a tuple as follows:

    {asn1_OPENTYPE,Binary}

Here Binary is an Erlang binary that contains the encoded data. (If option legacy_erlang_types has been given, only the binary is returned.)

### 3.10 Parameterization (X.683)

Parameterization, which is defined in X.683, can be used when defining types, values, value sets, classes, objects, or object sets. A part of a definition can be supplied as a parameter. For example, if a Type is used in a definition with a certain purpose, you want the type name to express the intention. This can be done with parameterization.

When many types (or another ASN.1 entity) only differ in some minor cases, but the structure of the types is similar, only one general type can be defined and the differences can be supplied through parameters.

Example of use of parameterization:

    General{Type} ::= SEQUENCE
    {
         number     INTEGER,
         string     Type
    }

    T1 ::= General{PrintableString}

    T2 ::= General{BIT STRING}

An example of a value that can be encoded as type T1 is {12,"hello"}.

Notice that the compiler does not generate encode/decode functions for parameterized types, only for the instances of the parameterized types. Therefore, if a file contains the types General{}, T1, and T2 as in the previous example, encode/decode functions are only generated for T1 and T2.