User's Guide
Reference Manual
Release Notes
PDF
Top

OTP_Mibs
Reference Manual
Version 1.1

Expand All
Contract All

Table of Contents

- otp_mib
  - Top of manual page
  - load/1
  - unload/1

# otp_mib

### MODULE

otp_mib

### MODULE SUMMARY

Handles the OTP-MIB

### DESCRIPTION

The SNMP application should be used to start an SNMP agent. Then the API functions below can be used to load/unload the OTP-MIB into/from the agent. The instrumentation of the OTP-MIB uses Mnesia, hence Mnesia must be started prior to loading the OTP-MIB.

### EXPORTS

load(Agent) -> ok | {error, Reason}

Types:

Agent = pid() | atom()
Reason = term()

Loads the OTP-MIB.

unload(Agent) -> ok | {error, Reason}

Types:

Agent = pid() | atom()
Reason = term()

Unloads the OTP-MIB.

### See Also

snmp(3)