User's Guide
Reference Manual
Release Notes
PDF
Top

Observer
User's Guide
Version 2.1.1

Expand All
Contract All

Chapters

- Observer
  - Top of chapter
  - Introduction
  - General
  - Applications
  - Processes
  - Table Viewer
  - Trace Overview
- Trace Tool Builder
  - Top of chapter
  - Introduction
  - Getting Started
  - Running the Trace Tool Builder against a remote node
  - Additional tracing options
  - Trace Information and the .ti File
  - Wrap Logs
  - Formatting
  - Automatically collect and format logs from all nodes
  - History and Configuration Files
  - Sequential Tracing
  - Example: Multipurpose trace tool
- Erlang Top
  - Top of chapter
  - Introduction
  - Output
  - Start
  - Configuration
  - Print to file
  - Stop
- Crashdump Viewer
  - Top of chapter
  - Introduction
  - Getting Started
  - The graphical interface
  - Data content
  - General information
  - Processes
  - Ports
  - ETS tables
  - Timers
  - Schedulers
  - Funs
  - Atoms
  - Nodes
  - Loaded modules
  - Memory
  - Internal tables

# 3 Erlang Top

### 3.1 Introduction

Erlang Top, etop is a tool for presenting information about erlang processes similar to the information presented by top in UNIX.

### 3.2 Output

The output from etop looks like this:

    ========================================================================================
     tiger@durin                                                               13:40:32
     Load:  cpu         0               Memory:  total        1997    binary         33
            procs     197                        processes       0    code          173
            runq      135                        atom         1002    ets            95

    Pid            Name or Initial Func    Time    Reds  Memory    MsgQ Current Function
    ----------------------------------------------------------------------------------------
    <127.23.0>     code_server                0   59585   78064       0 gen_server:loop/6
    <127.21.0>     file_server_2              0   36380   44276       0 gen_server:loop/6
    <127.2.0>      erl_prim_loader            0   27962    3740       0 erl_prim_loader:loop
    <127.9.0>      kernel_sup                 0    6998    4676       0 gen_server:loop/6
    <127.17.0>     net_kernel                62    6018    3136       0 gen_server:loop/6
    <127.0.0>      init                       0    4156    4352       0 init:loop/1
    <127.16.0>     auth                       0    1765    1264       0 gen_server:loop/6
    <127.18.0>     inet_tcp_dist:accept       0     660    1416       0 prim_inet:accept0/2
    <127.5.0>      application_controll       0     569    6756       0 gen_server:loop/6
    <127.137.0>    net_kernel:do_spawn_       0     553    5840       0 dbg:do_relay_1/1
    ========================================================================================

The header includes some system information:

Load
  cpu is Runtime/Wallclock, i.e. the percentage of time where the node has been active, procs is the number of processes on the node, and runq is the number of processes that are ready to run.
Memory
  This is the memory allocated by the node in kilo bytes.

For each process the following information is presented:

Time
  This is the runtime for the process, i.e. the actual time the process has been scheduled in.
Reds
  This is the number of reductions that has been executed on the process
Memory
  This is the size of the process in bytes, obtained by a call to process_info(Pid,memory).
MsgQ
  This is the length of the message queue for the process.

Note

Time and Reds can be presented as accumulated values or as values since last update.

### 3.3 Start

To start etop use the script etop or the batch file etop.bat, e.g. etop -node tiger@durin,

### 3.4 Configuration

All configuration parameters can be set at start by adding -OptName Value to the command line, e.g. etop -node tiger@durin -setcookie mycookie -lines 15.

The parameters lines, interval, accumulate and sort can be changed during runtime by the function etop:config/2.

A list of all valid configuration parameters can be found in the reference manual for etop.

#### Example: Change configuration with text based presentation

    ========================================================================================
     tiger@durin                                                               10:12:39
     Load:  cpu         0               Memory:  total        1858    binary         33
            procs     191                        processes       0    code          173
            runq        2                        atom         1002    ets            95

    Pid            Name or Initial Func    Time    Reds  Memory    MsgQ Current Function
    ----------------------------------------------------------------------------------------
    <127.23.0>     code_server                0   60350   71176       0 gen_server:loop/6
    <127.21.0>     file_server_2              0   36380   44276       0 gen_server:loop/6
    <127.2.0>      erl_prim_loader            0   27962    3740       0 erl_prim_loader:loop
    <127.17.0>     net_kernel                 0   13808    3916       0 gen_server:loop/6
    <127.9.0>      kernel_sup                 0    6998    4676       0 gen_server:loop/6
    <127.0.0>      init                       0    4156    4352       0 init:loop/1
    <127.18.0>     inet_tcp_dist:accept       0    2196    1416       0 prim_inet:accept0/2
    <127.16.0>     auth                       0    1893    1264       0 gen_server:loop/6
    <127.43.0>     ddll_server                0     582    3744       0 gen_server:loop/6
    <127.5.0>      application_controll       0     569    6756       0 gen_server:loop/6
    ========================================================================================

etop:config(lines,5).
ok

    (etop@durin)2>
    ========================================================================================
     tiger@durin                                                               10:12:44
     Load:  cpu         0               Memory:  total        1859    binary         33
            procs     192                        processes       0    code          173
            runq        2                        atom         1002    ets            95

    Pid            Name or Initial Func    Time    Reds  Memory    MsgQ Current Function
    ----------------------------------------------------------------------------------------
    <127.17.0>     net_kernel               183      70    4092       0 gen_server:loop/6
    <127.335.0>    inet_tcp_dist:do_acc     141      22    1856       0 dist_util:con_loop/9
    <127.19.0>     net_kernel:ticker/2      155       6    1244       0 net_kernel:ticker1/2
    <127.341.0>    net_kernel:do_spawn_       0       0    5840       0 dbg:do_relay_1/1
    <127.43.0>     ddll_server                0       0    3744       0 gen_server:loop/6
    ========================================================================================

### 3.5 Print to file

At any time, the current etop display can be dumped to a text file with the function etop:dump/1.

### 3.6 Stop

Use the function etop:stop/0 to stop etop.