User's Guide
Reference Manual
Release Notes
PDF
Top

cosNotification
Release Notes
Version 1.2

Expand All
Contract All

Chapters

- cosNotification Release Notes
  - Top of chapter
  - cosNotification 1.2
  - cosNotification 1.1.21
  - cosNotification 1.1.20
  - cosNotification 1.1.19
  - cosNotification 1.1.18
  - cosNotification 1.1.17
  - cosNotification 1.1.16
  - cosNotification 1.1.15
  - cosNotification 1.1.14
  - cosNotification 1.1.14
  - cosNotification 1.1.13
  - cosNotification 1.1.12
  - cosNotification 1.1.11
  - cosNotification 1.1.10
  - cosNotification 1.1.9
  - cosNotification 1.1.8
  - cosNotification 1.1.7
  - cosNotification 1.1.6
  - cosNotification 1.1.5
  - cosNotification 1.1.4
  - cosNotification 1.1.3
  - cosNotification 1.1.2
  - cosNotification 1.1.1
  - cosNotification 1.1
  - cosNotification 1.0.6
  - cosNotification 1.0.5
  - cosNotification 1.0.4
  - cosNotification 1.0.3
  - cosNotification 1.0.2

# 1 cosNotification Release Notes

### 1.1 cosNotification 1.2

#### Improvements and New Features

- Remove the usage of erlang:now() from all Corba applications and use the new rand module instead of random.

  Own Id: OTP-12687

### 1.2 cosNotification 1.1.21

#### Improvements and New Features

- The default encoding of Erlang files has been changed from ISO-8859-1 to UTF-8.

  The encoding of XML files has also been changed to UTF-8.

  Own Id: OTP-10907

### 1.3 cosNotification 1.1.20

#### Improvements and New Features

- Postscript files no longer needed for the generation of PDF files have been removed.

  Own Id: OTP-11016

### 1.4 cosNotification 1.1.19

#### Improvements and New Features

- Misc build updates

  Own Id: OTP-10784

### 1.5 cosNotification 1.1.18

#### Improvements and New Features

- Erlang/OTP can now be built using parallel make if you limit the number of jobs, for instance using 'make -j6' or 'make -j10'. 'make -j' does not work at the moment because of some missing dependencies.

  Own Id: OTP-9451

### 1.6 cosNotification 1.1.17

#### Improvements and New Features

- Removed superfluous usage of shy in the documentation since it can cause problem if a buggy tool is used.

  Own Id: OTP-9319 Aux Id:

### 1.7 cosNotification 1.1.16

#### Improvements and New Features

- Eliminated Dialyzer warnings when using exit or throw.

  Own Id: OTP-9050

### 1.8 cosNotification 1.1.15

#### Improvements and New Features

- Switched from using the deprecated regexp to re instead.

  Own Id: OTP-8846

### 1.9 cosNotification 1.1.14

#### Improvements and New Features

- Test suites published.

  Own Id: OTP-8543 Aux Id:

#### Fixed Bugs and Malfunctions

- Added missing trailing bracket to define in hrl-file.

  Own Id: OTP-8489 Aux Id:

### 1.10 cosNotification 1.1.14

#### Improvements and New Features

- Test suites published.

  Own Id: OTP-8543 Aux Id:

#### Fixed Bugs and Malfunctions

- Added missing trailing bracket to define in hrl-file.

  Own id: OTP-8489 Aux Id:

### 1.11 cosNotification 1.1.13

#### Fixed Bugs and Malfunctions

- Removed superfluous VT in the documentation.

  Own Id: OTP-8353 Aux Id:

- Removed superfluous backslash in the documentation.

  Own Id: OTP-8354 Aux Id:

- The documentation EIX file was not generated.

  Own Id: OTP-8355 Aux Id:

### 1.12 cosNotification 1.1.12

#### Improvements and New Features

- The documentation is now built with open source tools (xsltproc and fop) that exists on most platforms. One visible change is that the frames are removed.

  Own Id: OTP-8201 Aux Id:

### 1.13 cosNotification 1.1.11

#### Improvements and New Features

- Obsolete guards, e.g. record vs is_record, has been changed to avoid compiler warnings.

  Own Id: OTP-7987

### 1.14 cosNotification 1.1.10

#### Fixed Bugs and Malfunctions

- Updated file headers.

  Own Id: OTP-7837 Aux Id:

### 1.15 cosNotification 1.1.9

#### Fixed Bugs and Malfunctions

- Documentation source included in open source releases.

  Own Id: OTP-7595 Aux Id:

### 1.16 cosNotification 1.1.8

#### Fixed Bugs and Malfunctions

- The CosNotification proxy objects ignored the gcLimit option, instead the gcTime value was used.

  Own Id: OTP-7553 Aux Id:

### 1.17 cosNotification 1.1.7

#### Improvements and New Features

- Updated file headers.

  Own Id: OTP-7011

### 1.18 cosNotification 1.1.6

#### Improvements and New Features

- The documentation source has been converted from SGML to XML.

  Own Id: OTP-6754

### 1.19 cosNotification 1.1.5

#### Improvements and New Features

- Minor Makefile changes.

  Own Id: OTP-6701

### 1.20 cosNotification 1.1.4

#### Improvements and New Features

- Removed some unused code.

  Own Id: OTP-6527

### 1.21 cosNotification 1.1.3

#### Improvements and New Features

- A user can now define the QoS EventReliability to be Persistent. Note, this is only a lightweight version and events will be lost if a proxy is terminated.

  Own Id: OTP-5923

### 1.22 cosNotification 1.1.2

#### Improvements and New Features

- Possible to configure cosNotification not to type check, by invoking corba_object:is_a/2, supplied IOR:s. When a type check fails, the feedback has been improved.

  Own Id: OTP-5823 Aux Id: seq10143

### 1.23 cosNotification 1.1.1

#### Fixed Bugs and Malfunctions

- The app-file contained duplicated modules.

  Own Id: OTP-4976

### 1.24 cosNotification 1.1

#### Improvements and New Features

- The stub/skeleton-files generated by IC have been improved, i.e., depending on the IDL-files, reduced the size of the erl- and beam-files and decreased dependencies off Orber's Interface Repository. It is necessary to re-compile all IDL-files and use COS-applications, including Orber, compiled with IC-4.2.

  Own Id: OTP-4576

### 1.25 cosNotification 1.0.6

#### Fixed Bugs and Malfunctions

- The exception CosNotifyFilter::InvalidValue, raised by the operation CosNotifyFilter::MappingFilter::add_mapping_constraints, did not contain correct data in the body. Hence, it was not possible to pass this exception to another ORB.

  Own Id: OTP-4412

- It was not possible to set the QoS property PacingInterval to zero and the default value was not compliant with the OMG specification. The default value for MaximumBatchSize have also been changed du to the same reason.

  Own Id: OTP-4413, OTP-4414

#### Incompatibilities

- The default value, for the QoS properties PacingInterval and MaximumBatchSize, have been changed to zero (i.e. no timeout) and 1 respectively, which is compliant with the OMG specification.

  Own Id: OTP-4413, OTP-4414

### 1.26 cosNotification 1.0.5

#### Fixed Bugs and Malfunctions

- If one tries to set an unavailable/incorrect property or property value, an exception is thrown. In some cases the exception was not correct, which would cause problems if communicating via IIOP.

  Own Id: OTP-4340

- When using Filter's, with the QoS OrderPolicy set to FifoOrder, and passing a sequence of structured events, they could be delivered in the wrong order.

  Own Id: OTP-4272

- If Filter's where attached to Supplier proxies it could cause the Proxy to terminate.

  Own Id: OTP-4272

### 1.27 cosNotification 1.0.4

#### Fixed Bugs and Malfunctions

- When passing event sequences, the PushSuppliers and PullSuppliers could crash if the objects had Filter objects associated and only a subset of the sequences where approved.

  Own Id: OTP-4099

- SupplierAdmin's did not filter any events, even though Filter objects had been attached to the SupplierAdmin.

  Own Id: OTP-4098

- If one used the '_get_default_supplier_admin'/1, exported by the CosNotifyChannelAdmin_EventChannel-module, it resulted in a loop which overloaded the channel. This is no longer the case.

  Own Id: OTP-4086

- If one used the '_get_default_filter_factory'/1, exported by the CosNotifyChannelAdmin_EventChannel-module, a new instance was created each time. Now fixed.

  Own Id: OTP-4092

#### Incompatibilities

- The include paths for CosNotification.idl have been changed. Hence, if you include this file in your own IDL-files you must update your paths to also point to where the cosEvent IDL-files are stored.

  Own Id: OTP-4093

### 1.28 cosNotification 1.0.3

#### Improvements and New Features

- It is now possible to start global channel factories.

  Own Id: OTP-4078

- The Orber, version 3.2.5 or later, configuration parameter orber_debug_level can now be used to generate reports when abnormal situations occurs. For more information consult the Orber User's Guide. Note, it is not recommended to use this option for delivered systems since some of the reports is not to be considered as errors. The value of orber_debug_level must be 3, or higher, for reports to be generated.

  Own Id: OTP-4077, OTP-3962

#### Fixed Bugs and Malfunctions

- When using the cosEvent API accessing a cosNotification admins the objects returned by the functions obtain_push_supplier, obtain_pull_supplier, obtain_push_consumer and obtain_pull_consumer was not of the correct type. Due to the interface change it is not possible to upgrade during runtime.

  Own Id: OTP-4079

### 1.29 cosNotification 1.0.2

#### Improvements and New Features

- First release of the cosNotification application.

  Own Id: -